#MicroXplorer Configuration settings - do not modify
ADC1.Channel-0\#ChannelRegularConversion=ADC_CHANNEL_TEMPSENSOR_ADC1
ADC1.ClockPrescaler=ADC_CLOCK_ASYNC_DIV8
ADC1.CommonPathInternal=null|ADC_CHANNEL_TEMPSENSOR_ADC1|null|null
ADC1.ContinuousConvMode=ENABLE
ADC1.DMAContinuousRequests=ENABLE
ADC1.ExternalTrigConv=ADC_EXTERNALTRIG_T15_TRGO
ADC1.IPParameters=Rank-0\#ChannelRegularConversion,master,Channel-0\#ChannelRegularConversion,SamplingTime-0\#ChannelRegularConversion,OffsetNumber-0\#ChannelRegularConversion,NbrOfConversionFlag,ClockPrescaler,ContinuousConvMode,DMAContinuousRequests,ExternalTrigConv,CommonPathInternal
ADC1.NbrOfConversionFlag=1
ADC1.OffsetNumber-0\#ChannelRegularConversion=ADC_OFFSET_NONE
ADC1.Rank-0\#ChannelRegularConversion=1
ADC1.SamplingTime-0\#ChannelRegularConversion=ADC_SAMPLETIME_640CYCLES_5
ADC1.master=1
ADC2.Channel-6\#ChannelRegularConversion=ADC_CHANNEL_13
ADC2.ClockPrescaler=ADC_CLOCK_ASYNC_DIV8
ADC2.CommonPathInternal=null|null|null|null
ADC2.ExternalTrigConv=ADC_EXTERNALTRIG_T3_TRGO
ADC2.IPParameters=Rank-6\#ChannelRegularConversion,Channel-6\#ChannelRegularConversion,SamplingTime-6\#ChannelRegularConversion,OffsetNumber-6\#ChannelRegularConversion,NbrOfConversionFlag,ClockPrescaler,ExternalTrigConv,Resolution,CommonPathInternal
ADC2.NbrOfConversionFlag=1
ADC2.OffsetNumber-6\#ChannelRegularConversion=ADC_OFFSET_NONE
ADC2.Rank-6\#ChannelRegularConversion=1
ADC2.Resolution=ADC_RESOLUTION_8B
ADC2.SamplingTime-6\#ChannelRegularConversion=ADC_SAMPLETIME_247CYCLES_5
CAD.formats=
CAD.pinconfig=
CAD.provider=
COMP4.Hysteresis=COMP_HYSTERESIS_70MV
COMP4.IPParameters=Hysteresis
DAC1.DAC_HighFrequency_OUT1-DAC_OUT1=DAC_HIGH_FREQUENCY_INTERFACE_MODE_ABOVE_160MHZ
DAC1.IPParameters=DAC_HighFrequency_OUT1-DAC_OUT1
Dma.ADC1.0.Direction=DMA_PERIPH_TO_MEMORY
Dma.ADC1.0.EventEnable=DISABLE
Dma.ADC1.0.Instance=DMA1_Channel2
Dma.ADC1.0.MemDataAlignment=DMA_MDATAALIGN_HALFWORD
Dma.ADC1.0.MemInc=DMA_MINC_ENABLE
Dma.ADC1.0.Mode=DMA_CIRCULAR
Dma.ADC1.0.PeriphDataAlignment=DMA_PDATAALIGN_HALFWORD
Dma.ADC1.0.PeriphInc=DMA_PINC_DISABLE
Dma.ADC1.0.Polarity=HAL_DMAMUX_REQ_GEN_RISING
Dma.ADC1.0.Priority=DMA_PRIORITY_LOW
Dma.ADC1.0.RequestNumber=1
Dma.ADC1.0.RequestParameters=Instance,Direction,PeriphInc,MemInc,PeriphDataAlignment,MemDataAlignment,Mode,Priority,SignalID,Polarity,RequestNumber,SyncSignalID,SyncPolarity,SyncEnable,EventEnable,SyncRequestNumber
Dma.ADC1.0.SignalID=NONE
Dma.ADC1.0.SyncEnable=DISABLE
Dma.ADC1.0.SyncPolarity=HAL_DMAMUX_SYNC_NO_EVENT
Dma.ADC1.0.SyncRequestNumber=1
Dma.ADC1.0.SyncSignalID=NONE
Dma.ADC2.1.Direction=DMA_PERIPH_TO_MEMORY
Dma.ADC2.1.EventEnable=DISABLE
Dma.ADC2.1.Instance=DMA1_Channel1
Dma.ADC2.1.MemDataAlignment=DMA_MDATAALIGN_BYTE
Dma.ADC2.1.MemInc=DMA_MINC_ENABLE
Dma.ADC2.1.Mode=DMA_NORMAL
Dma.ADC2.1.PeriphDataAlignment=DMA_PDATAALIGN_BYTE
Dma.ADC2.1.PeriphInc=DMA_PINC_DISABLE
Dma.ADC2.1.Polarity=HAL_DMAMUX_REQ_GEN_RISING
Dma.ADC2.1.Priority=DMA_PRIORITY_VERY_HIGH
Dma.ADC2.1.RequestNumber=1
Dma.ADC2.1.RequestParameters=Instance,Direction,PeriphInc,MemInc,PeriphDataAlignment,MemDataAlignment,Mode,Priority,SignalID,Polarity,RequestNumber,SyncSignalID,SyncPolarity,SyncEnable,EventEnable,SyncRequestNumber
Dma.ADC2.1.SignalID=NONE
Dma.ADC2.1.SyncEnable=DISABLE
Dma.ADC2.1.SyncPolarity=HAL_DMAMUX_SYNC_NO_EVENT
Dma.ADC2.1.SyncRequestNumber=1
Dma.ADC2.1.SyncSignalID=NONE
Dma.Request0=ADC1
Dma.Request1=ADC2
Dma.RequestsNb=2
FDCAN1.AutoRetransmission=ENABLE
FDCAN1.CalculateBaudRateNominal=500000
FDCAN1.CalculateTimeBitNominal=2000
FDCAN1.CalculateTimeQuantumNominal=125.0
FDCAN1.DataSyncJumpWidth=1
FDCAN1.DataTimeSeg1=1
FDCAN1.DataTimeSeg2=1
FDCAN1.FrameFormat=FDCAN_FRAME_CLASSIC
FDCAN1.IPParameters=CalculateTimeQuantumNominal,CalculateTimeBitNominal,CalculateBaudRateNominal,FrameFormat,AutoRetransmission,TransmitPause,NominalSyncJumpWidth,DataSyncJumpWidth,DataTimeSeg1,StdFiltersNbr,DataTimeSeg2,NominalPrescaler,NominalTimeSeg1,NominalTimeSeg2
FDCAN1.NominalPrescaler=20
FDCAN1.NominalSyncJumpWidth=2
FDCAN1.NominalTimeSeg1=13
FDCAN1.NominalTimeSeg2=2
FDCAN1.StdFiltersNbr=1
FDCAN1.TransmitPause=ENABLE
File.Version=6
GPIO.groupedBy=Group By Peripherals
KeepUserPlacement=false
Mcu.CPN=STM32G431KBU6
Mcu.Family=STM32G4
Mcu.IP0=ADC1
Mcu.IP1=ADC2
Mcu.IP10=RTC
Mcu.IP11=SYS
Mcu.IP12=TIM1
Mcu.IP13=TIM2
Mcu.IP14=TIM3
Mcu.IP15=TIM4
Mcu.IP16=TIM6
Mcu.IP17=TIM7
Mcu.IP18=TIM8
Mcu.IP19=TIM15
Mcu.IP2=COMP4
Mcu.IP20=TIM16
Mcu.IP21=TIM17
Mcu.IP22=USART1
Mcu.IP3=DAC1
Mcu.IP4=DMA
Mcu.IP5=FDCAN1
Mcu.IP6=NVIC
Mcu.IP7=OPAMP1
Mcu.IP8=OPAMP2
Mcu.IP9=RCC
Mcu.IPNb=23
Mcu.Name=STM32G431K(6-8-B)Ux
Mcu.Package=UFQFPN32
Mcu.Pin0=PF0-OSC_IN
Mcu.Pin1=PF1-OSC_OUT
Mcu.Pin10=PA9
Mcu.Pin11=PA10
Mcu.Pin12=PA11
Mcu.Pin13=PA12
Mcu.Pin14=PA13
Mcu.Pin15=PA14
Mcu.Pin16=PA15
Mcu.Pin17=PB3
Mcu.Pin18=PB4
Mcu.Pin19=PB6
Mcu.Pin2=PA0
Mcu.Pin20=PB7
Mcu.Pin21=PB8-BOOT0
Mcu.Pin22=VP_ADC1_TempSens_Input
Mcu.Pin23=VP_COMP4_VS_VREFINT14
Mcu.Pin24=VP_RTC_VS_RTC_Activate
Mcu.Pin25=VP_RTC_VS_RTC_WakeUp_intern
Mcu.Pin26=VP_SYS_VS_Systick
Mcu.Pin27=VP_SYS_VS_DBSignals
Mcu.Pin28=VP_TIM1_VS_ClockSourceINT
Mcu.Pin29=VP_TIM1_VS_no_output3
Mcu.Pin3=PA2
Mcu.Pin30=VP_TIM1_VS_OPM
Mcu.Pin31=VP_TIM2_VS_ClockSourceINT
Mcu.Pin32=VP_TIM2_VS_NoInput3
Mcu.Pin33=VP_TIM3_VS_ControllerModeGated
Mcu.Pin34=VP_TIM3_VS_ClockSourceINT
Mcu.Pin35=VP_TIM3_VS_ClockSourceITR
Mcu.Pin36=VP_TIM4_VS_ClockSourceINT
Mcu.Pin37=VP_TIM6_VS_ClockSourceINT
Mcu.Pin38=VP_TIM7_VS_ClockSourceINT
Mcu.Pin39=VP_TIM8_VS_no_output1
Mcu.Pin4=PA3
Mcu.Pin40=VP_TIM15_VS_ClockSourceINT
Mcu.Pin41=VP_TIM16_VS_ClockSourceINT
Mcu.Pin42=VP_TIM17_VS_ClockSourceINT
Mcu.Pin43=VP_TIM17_VS_OPM
Mcu.Pin5=PA4
Mcu.Pin6=PA5
Mcu.Pin7=PA6
Mcu.Pin8=PA7
Mcu.Pin9=PB0
Mcu.PinsNb=44
Mcu.ThirdPartyNb=0
Mcu.UserConstants=
Mcu.UserName=STM32G431KBUx
MxCube.Version=6.13.0
MxDb.Version=DB.6.0.130
NVIC.BusFault_IRQn=true\:0\:0\:false\:false\:true\:false\:false\:false
NVIC.DMA1_Channel1_IRQn=true\:0\:0\:false\:false\:true\:false\:true\:true
NVIC.DMA1_Channel2_IRQn=true\:7\:0\:true\:false\:true\:false\:true\:true
NVIC.DebugMonitor_IRQn=true\:0\:0\:false\:false\:true\:false\:false\:false
NVIC.FDCAN1_IT0_IRQn=true\:2\:0\:true\:false\:true\:true\:true\:true
NVIC.ForceEnableDMAVector=true
NVIC.HardFault_IRQn=true\:0\:0\:false\:false\:true\:false\:false\:false
NVIC.MemoryManagement_IRQn=true\:0\:0\:false\:false\:true\:false\:false\:false
NVIC.NonMaskableInt_IRQn=true\:0\:0\:false\:false\:true\:false\:false\:false
NVIC.PendSV_IRQn=true\:0\:0\:false\:false\:true\:false\:false\:false
NVIC.PriorityGroup=NVIC_PRIORITYGROUP_4
NVIC.RTC_WKUP_IRQn=true\:13\:0\:true\:false\:true\:true\:true\:true
NVIC.SVCall_IRQn=true\:0\:0\:false\:false\:true\:false\:false\:false
NVIC.SysTick_IRQn=true\:15\:0\:false\:false\:true\:false\:true\:false
NVIC.TIM1_BRK_TIM15_IRQn=true\:5\:0\:true\:false\:true\:true\:true\:true
NVIC.TIM1_CC_IRQn=true\:0\:0\:true\:false\:true\:true\:true\:true
NVIC.TIM1_TRG_COM_TIM17_IRQn=true\:0\:0\:false\:false\:true\:true\:true\:true
NVIC.TIM2_IRQn=true\:1\:0\:true\:false\:true\:true\:true\:true
NVIC.TIM3_IRQn=true\:2\:0\:true\:false\:true\:true\:true\:true
NVIC.TIM6_DAC_IRQn=true\:4\:0\:true\:false\:true\:true\:true\:true
NVIC.USART1_IRQn=true\:5\:0\:true\:false\:true\:true\:true\:true
NVIC.UsageFault_IRQn=true\:0\:0\:false\:false\:true\:false\:false\:false
PA0.Signal=S_TIM2_CH1
PA10.GPIOParameters=GPIO_ModeDefaultPP,GPIO_Speed,GPIO_PuPd
PA10.GPIO_ModeDefaultPP=GPIO_MODE_AF_PP
PA10.GPIO_PuPd=GPIO_NOPULL
PA10.GPIO_Speed=GPIO_SPEED_FREQ_LOW
PA10.Mode=Asynchronous
PA10.Signal=USART1_RX
PA11.Mode=FDCAN_Activate
PA11.Signal=FDCAN1_RX
PA12.Mode=FDCAN_Activate
PA12.Signal=FDCAN1_TX
PA13.Mode=Serial_Wire
PA13.Signal=SYS_JTMS-SWDIO
PA14.Mode=Serial_Wire
PA14.Signal=SYS_JTCK-SWCLK
PA15.GPIOParameters=GPIO_Speed,GPIO_Label
PA15.GPIO_Label=SYNC_OUT
PA15.GPIO_Speed=GPIO_SPEED_FREQ_VERY_HIGH
PA15.Locked=true
PA15.Signal=GPIO_Output
PA2.Mode=Follower
PA2.Signal=OPAMP1_VOUT
PA3.Locked=true
PA3.Mode=Follower
PA3.Signal=OPAMP1_VINP
PA4.GPIOParameters=GPIO_Label
PA4.GPIO_Label=DAC_PEAK
PA4.Signal=COMP_DAC11_group
PA5.GPIOParameters=GPIO_Label
PA5.GPIO_Label=ADC_TEIN
PA5.Mode=IN13-Single-Ended
PA5.Signal=ADC2_IN13
PA6.Mode=Follower
PA6.Signal=OPAMP2_VOUT
PA7.Locked=true
PA7.Mode=Follower
PA7.Signal=OPAMP2_VINP
PA9.GPIOParameters=GPIO_ModeDefaultPP,GPIO_Speed,GPIO_PuPd
PA9.GPIO_ModeDefaultPP=GPIO_MODE_AF_PP
PA9.GPIO_PuPd=GPIO_NOPULL
PA9.GPIO_Speed=GPIO_SPEED_FREQ_HIGH
PA9.Mode=Asynchronous
PA9.Signal=USART1_TX
PB0.GPIOParameters=GPIO_Label
PB0.GPIO_Label=IN_CKP
PB0.Locked=true
PB0.Mode=INP
PB0.Signal=COMP4_INP
PB3.GPIOParameters=GPIO_PuPd,GPIO_Label
PB3.GPIO_Label=IDLE_IN
PB3.GPIO_PuPd=GPIO_PULLDOWN
PB3.Locked=true
PB3.Signal=GPIO_Input
PB4.GPIOParameters=GPIO_PuPd,GPIO_Label
PB4.GPIO_Label=SHUT_OFF
PB4.GPIO_PuPd=GPIO_PULLDOWN
PB4.Locked=true
PB4.Signal=GPIO_Input
PB6.GPIOParameters=GPIO_FM6,GPIO_Speed,GPIO_PuPd,GPIO_Label
PB6.GPIO_FM6=SYSCFG_FASTMODEPLUS_PB6
PB6.GPIO_Label=HOLD_CONTROL
PB6.GPIO_PuPd=GPIO_PULLDOWN
PB6.GPIO_Speed=GPIO_SPEED_FREQ_VERY_HIGH
PB6.Locked=true
PB6.Signal=GPIO_Output
PB7.GPIOParameters=GPIO_Label
PB7.GPIO_Label=ADVANCE_PWM
PB7.Locked=true
PB7.Signal=S_TIM4_CH2
PB8-BOOT0.Locked=true
PF0-OSC_IN.Mode=HSE-External-Oscillator
PF0-OSC_IN.Signal=RCC_OSC_IN
PF1-OSC_OUT.Mode=HSE-External-Oscillator
PF1-OSC_OUT.Signal=RCC_OSC_OUT
PinOutPanel.RotationAngle=0
ProjectManager.AskForMigrate=true
ProjectManager.BackupPrevious=false
ProjectManager.CompilerOptimize=6
ProjectManager.ComputerToolchain=false
ProjectManager.CoupleFile=false
ProjectManager.CustomerFirmwarePackage=
ProjectManager.DefaultFWLocation=true
ProjectManager.DeletePrevious=true
ProjectManager.DeviceId=STM32G431KBUx
ProjectManager.FirmwarePackage=STM32Cube FW_G4 V1.6.1
ProjectManager.FreePins=false
ProjectManager.HalAssertFull=false
ProjectManager.HeapSize=0x200
ProjectManager.KeepUserCode=true
ProjectManager.LastFirmware=false
ProjectManager.LibraryCopy=1
ProjectManager.MainLocation=Core/Src
ProjectManager.NoMain=false
ProjectManager.PreviousToolchain=STM32CubeIDE
ProjectManager.ProjectBuild=false
ProjectManager.ProjectFileName=hpsg5-controller_v2-stm32g4.ioc
ProjectManager.ProjectName=hpsg5-controller_v2-stm32g4
ProjectManager.ProjectStructure=
ProjectManager.RegisterCallBack=
ProjectManager.StackSize=0x400
ProjectManager.TargetToolchain=STM32CubeIDE
ProjectManager.ToolChainLocation=
ProjectManager.UAScriptAfterPath=
ProjectManager.UAScriptBeforePath=
ProjectManager.UnderRoot=true
ProjectManager.functionlistsort=1-SystemClock_Config-RCC-false-HAL-false,2-MX_GPIO_Init-GPIO-false-HAL-true,3-MX_DMA_Init-DMA-false-HAL-true,4-MX_ADC1_Init-ADC1-false-HAL-true,5-MX_ADC2_Init-ADC2-false-HAL-true,6-MX_COMP4_Init-COMP4-false-HAL-true,7-MX_DAC1_Init-DAC1-false-HAL-true,8-MX_FDCAN1_Init-FDCAN1-false-HAL-true,9-MX_OPAMP1_Init-OPAMP1-false-HAL-true,10-MX_TIM2_Init-TIM2-false-HAL-true,11-MX_TIM4_Init-TIM4-false-HAL-true,12-MX_USART1_UART_Init-USART1-false-HAL-true,13-MX_TIM1_Init-TIM1-false-HAL-true,14-MX_TIM3_Init-TIM3-false-HAL-true,15-MX_TIM6_Init-TIM6-false-HAL-true,16-MX_TIM7_Init-TIM7-false-HAL-true,17-MX_TIM15_Init-TIM15-false-HAL-true,18-MX_TIM16_Init-TIM16-false-HAL-true,19-MX_RTC_Init-RTC-false-HAL-true,20-MX_TIM8_Init-TIM8-false-HAL-true,21-MX_OPAMP2_Init-OPAMP2-false-HAL-true,22-MX_TIM17_Init-TIM17-false-HAL-true
RCC.ADC12Freq_Value=160000000
RCC.AHBFreq_Value=160000000
RCC.APB1Freq_Value=160000000
RCC.APB1TimFreq_Value=160000000
RCC.APB2Freq_Value=160000000
RCC.APB2TimFreq_Value=160000000
RCC.CRSFreq_Value=48000000
RCC.CortexFreq_Value=160000000
RCC.EXTERNAL_CLOCK_VALUE=12288000
RCC.FCLKCortexFreq_Value=160000000
RCC.FDCANFreq_Value=160000000
RCC.FamilyName=M
RCC.HCLKFreq_Value=160000000
RCC.HSE_VALUE=16000000
RCC.HSI48_VALUE=48000000
RCC.HSI_VALUE=16000000
RCC.I2C1Freq_Value=160000000
RCC.I2C2Freq_Value=160000000
RCC.I2C3Freq_Value=160000000
RCC.I2SFreq_Value=160000000
RCC.IPParameters=ADC12Freq_Value,AHBFreq_Value,APB1Freq_Value,APB1TimFreq_Value,APB2Freq_Value,APB2TimFreq_Value,CRSFreq_Value,CortexFreq_Value,EXTERNAL_CLOCK_VALUE,FCLKCortexFreq_Value,FDCANFreq_Value,FamilyName,HCLKFreq_Value,HSE_VALUE,HSI48_VALUE,HSI_VALUE,I2C1Freq_Value,I2C2Freq_Value,I2C3Freq_Value,I2SFreq_Value,LPTIM1Freq_Value,LPUART1Freq_Value,LSCOPinFreq_Value,LSE_VALUE,LSI_VALUE,MCO1PinFreq_Value,PLLN,PLLPoutputFreq_Value,PLLQoutputFreq_Value,PLLRCLKFreq_Value,PLLSourceVirtual,PWRFreq_Value,RNGFreq_Value,SAI1Freq_Value,SYSCLKFreq_VALUE,SYSCLKSource,USART1Freq_Value,USART2Freq_Value,USBFreq_Value,VCOInputFreq_Value,VCOOutputFreq_Value
RCC.LPTIM1Freq_Value=160000000
RCC.LPUART1Freq_Value=160000000
RCC.LSCOPinFreq_Value=32000
RCC.LSE_VALUE=32768
RCC.LSI_VALUE=32000
RCC.MCO1PinFreq_Value=16000000
RCC.PLLN=20
RCC.PLLPoutputFreq_Value=160000000
RCC.PLLQoutputFreq_Value=160000000
RCC.PLLRCLKFreq_Value=160000000
RCC.PLLSourceVirtual=RCC_PLLSOURCE_HSE
RCC.PWRFreq_Value=160000000
RCC.RNGFreq_Value=160000000
RCC.SAI1Freq_Value=160000000
RCC.SYSCLKFreq_VALUE=160000000
RCC.SYSCLKSource=RCC_SYSCLKSOURCE_PLLCLK
RCC.USART1Freq_Value=160000000
RCC.USART2Freq_Value=160000000
RCC.USBFreq_Value=160000000
RCC.VCOInputFreq_Value=16000000
RCC.VCOOutputFreq_Value=320000000
RTC.HourFormat=RTC_HOURFORMAT_24
RTC.IPParameters=HourFormat,WakeUpClock,WakeUpCounter
RTC.WakeUpClock=RTC_WAKEUPCLOCK_CK_SPRE_16BITS
RTC.WakeUpCounter=900
SH.COMP_DAC11_group.0=DAC1_OUT1,DAC_OUT1
SH.COMP_DAC11_group.ConfNb=1
SH.S_TIM2_CH1.0=TIM2_CH1,Input_Capture1_from_TI1
SH.S_TIM2_CH1.ConfNb=1
SH.S_TIM4_CH2.0=TIM4_CH2,PWM Generation2 CH2
SH.S_TIM4_CH2.ConfNb=1
TIM1.Channel-PWM\ Generation3\ No\ Output=TIM_CHANNEL_3
TIM1.IPParameters=Channel-PWM Generation3 No Output,Prescaler,PulseNoDither_3,TIM_MasterOutputTrigger
TIM1.Prescaler=20-1
TIM1.PulseNoDither_3=1000
TIM1.TIM_MasterOutputTrigger=TIM_TRGO_OC3REF
TIM15.IPParameters=Prescaler,PeriodNoDither,TIM_MasterOutputTrigger
TIM15.PeriodNoDither=1000
TIM15.Prescaler=160-1
TIM15.TIM_MasterOutputTrigger=TIM_TRGO_UPDATE
TIM16.IPParameters=Prescaler
TIM16.Prescaler=16000-1
TIM17.IPParameters=Prescaler,PeriodNoDither
TIM17.PeriodNoDither=65535
TIM17.Prescaler=160-1
TIM2.Channel-Input_Capture1_from_TI1=TIM_CHANNEL_1
TIM2.Channel-Input_Capture3_from_TI3_Remap_TIM2=TIM_CHANNEL_3
TIM2.ICFilter_CH1=15
TIM2.ICFilter_CH3=2
TIM2.ICPolarity_CH1=TIM_INPUTCHANNELPOLARITY_FALLING
TIM2.ICPolarity_CH3=TIM_INPUTCHANNELPOLARITY_FALLING
TIM2.IPParameters=Prescaler,ICPolarity_CH1,ICFilter_CH1,Channel-Input_Capture3_from_TI3_Remap_TIM2,ICPolarity_CH3,ICFilter_CH3,Channel-Input_Capture1_from_TI1
TIM2.Prescaler=10-1
TIM3.IPParameters=Prescaler,PeriodNoDither,TIM_MasterOutputTrigger
TIM3.PeriodNoDither=16-1
TIM3.Prescaler=160-1
TIM3.TIM_MasterOutputTrigger=TIM_TRGO_UPDATE
TIM4.Channel-PWM\ Generation2\ CH2=TIM_CHANNEL_2
TIM4.IPParameters=Channel-PWM Generation2 CH2,Prescaler,PeriodNoDither,PulseNoDither_2
TIM4.PeriodNoDither=20000
TIM4.Prescaler=160-1
TIM4.PulseNoDither_2=5000
TIM6.IPParameters=Prescaler,PeriodNoDither
TIM6.PeriodNoDither=10000-1
TIM6.Prescaler=160-1
TIM7.IPParameters=Prescaler,PeriodNoDither,TIM_MasterOutputTrigger
TIM7.PeriodNoDither=9
TIM7.Prescaler=15
TIM7.TIM_MasterOutputTrigger=TIM_TRGO_UPDATE
TIM8.Channel-PWM\ Generation1\ No\ Output=TIM_CHANNEL_1
TIM8.IPParameters=Channel-PWM Generation1 No Output,Prescaler,PeriodNoDither,PulseNoDither_1
TIM8.PeriodNoDither=999
TIM8.Prescaler=8000-1
TIM8.PulseNoDither_1=199
USART1.IPParameters=VirtualMode-Asynchronous
USART1.VirtualMode-Asynchronous=VM_ASYNC
VP_ADC1_TempSens_Input.Mode=IN-TempSens
VP_ADC1_TempSens_Input.Signal=ADC1_TempSens_Input
VP_COMP4_VS_VREFINT14.Mode=VREFINT_14
VP_COMP4_VS_VREFINT14.Signal=COMP4_VS_VREFINT14
VP_RTC_VS_RTC_Activate.Mode=RTC_Enabled
VP_RTC_VS_RTC_Activate.Signal=RTC_VS_RTC_Activate
VP_RTC_VS_RTC_WakeUp_intern.Mode=WakeUp
VP_RTC_VS_RTC_WakeUp_intern.Signal=RTC_VS_RTC_WakeUp_intern
VP_SYS_VS_DBSignals.Mode=DisableDeadBatterySignals
VP_SYS_VS_DBSignals.Signal=SYS_VS_DBSignals
VP_SYS_VS_Systick.Mode=SysTick
VP_SYS_VS_Systick.Signal=SYS_VS_Systick
VP_TIM15_VS_ClockSourceINT.Mode=Internal
VP_TIM15_VS_ClockSourceINT.Signal=TIM15_VS_ClockSourceINT
VP_TIM16_VS_ClockSourceINT.Mode=Enable_Timer
VP_TIM16_VS_ClockSourceINT.Signal=TIM16_VS_ClockSourceINT
VP_TIM17_VS_ClockSourceINT.Mode=Enable_Timer
VP_TIM17_VS_ClockSourceINT.Signal=TIM17_VS_ClockSourceINT
VP_TIM17_VS_OPM.Mode=OPM_bit
VP_TIM17_VS_OPM.Signal=TIM17_VS_OPM
VP_TIM1_VS_ClockSourceINT.Mode=Internal
VP_TIM1_VS_ClockSourceINT.Signal=TIM1_VS_ClockSourceINT
VP_TIM1_VS_OPM.Mode=OPM_bit
VP_TIM1_VS_OPM.Signal=TIM1_VS_OPM
VP_TIM1_VS_no_output3.Mode=PWM Generation3 No Output
VP_TIM1_VS_no_output3.Signal=TIM1_VS_no_output3
VP_TIM2_VS_ClockSourceINT.Mode=Internal
VP_TIM2_VS_ClockSourceINT.Signal=TIM2_VS_ClockSourceINT
VP_TIM2_VS_NoInput3.Mode=Input_Capture3_from_TI3_Remap_TIM2
VP_TIM2_VS_NoInput3.Signal=TIM2_VS_NoInput3
VP_TIM3_VS_ClockSourceINT.Mode=Internal
VP_TIM3_VS_ClockSourceINT.Signal=TIM3_VS_ClockSourceINT
VP_TIM3_VS_ClockSourceITR.Mode=TriggerSource_ITR0
VP_TIM3_VS_ClockSourceITR.Signal=TIM3_VS_ClockSourceITR
VP_TIM3_VS_ControllerModeGated.Mode=Gated Mode
VP_TIM3_VS_ControllerModeGated.Signal=TIM3_VS_ControllerModeGated
VP_TIM4_VS_ClockSourceINT.Mode=Internal
VP_TIM4_VS_ClockSourceINT.Signal=TIM4_VS_ClockSourceINT
VP_TIM6_VS_ClockSourceINT.Mode=Enable_Timer
VP_TIM6_VS_ClockSourceINT.Signal=TIM6_VS_ClockSourceINT
VP_TIM7_VS_ClockSourceINT.Mode=Enable_Timer
VP_TIM7_VS_ClockSourceINT.Signal=TIM7_VS_ClockSourceINT
VP_TIM8_VS_no_output1.Mode=PWM Generation1 No Output
VP_TIM8_VS_no_output1.Signal=TIM8_VS_no_output1
board=custom
isbadioc=false
